Version: 1


Lab 1 Configuration of MyPBX

Preparation: Open a browser (e.g. google chrome or firefox), type in 192.168.5.150. You will see the landing page of MyPBX. You will need the following to access the system.

Username: admin, Password: P@ssw0rd01


Part 1: General Preference & DHCP Server

Under system, enable the DHCP running with the network of 192.168.5.2-254 subnet 255.255.255.0. Set the router as 192.168.5.1.



Click at the PBX button at top right hand corner and the main page of MyPBX will appear.

Set the following preferences or change them if necessary. The user extensions and etc can be changed to suit the requirements of users.



Part 2: Adding extension

On the left panel, click at the FXS/VOIP Extension and this will allow the configuration of new extension. Use “Add Extensions” or “Add bulk extensions” to create new extension numbers.

At this stage, you should set the password of the account you want to join from the IP phone.


For example, if you want the phone to join account 301, from the IP phone, key in the password as set in the IVR.

Part 3: Setting of Conference

Select “conferences” on the left panel. Password can be added to for participants to join the conference call.

Part 4: Setting of IVR

Again on the left panel, click at IVR under the Inboud call control. Give a number e.g. 660 to the IVR and also action for each answer from the caller.



Part 5: Setting of Ring Group

